From fe90ae8a9f54e4fe8b9089fed48b0e1818414f57 Mon Sep 17 00:00:00 2001
From: Alan Modra <amodra@gmail.com>
Date: Fri, 20 Mar 2020 10:51:14 +1030
Subject: [PATCH] NDS32 disassembly of odd sized sections

	* nds32-dis.c (print_insn_nds32): Remove unnecessary casts.
	Initialize parts of buffer not written when handling a possible
	2-byte insn at end of section.  Don't attempt decoding of such
	an insn by the 4-byte machinery.
---
 opcodes/nds32-dis.c | 24 +++++++++++++++---------
 1 files changed, 15 insertions(+), 9 deletions(-)

diff --git a/opcodes/nds32-dis.c b/opcodes/nds32-dis.c
index c5874ff..35e4ba0 100644
--- a/opcodes/nds32-dis.c
+++ b/opcodes/nds32-dis.c
@@ -985,7 +985,7 @@ print_insn_nds32 (bfd_vma pc, disassemble_info *info)
   int is_data = FALSE;
   bfd_boolean found = FALSE;
   struct nds32_private_data *private_data;
-  unsigned int size = 16;
+  unsigned int size;
   enum map_type mapping_type = MAP_CODE;
 
   if (info->private_data == NULL)
@@ -1063,6 +1063,7 @@ print_insn_nds32 (bfd_vma pc, disassemble_info *info)
 
       /* Fix corner case: there is no next mapping symbol,
 	 let mapping type decides size */
+      size = 16;
       if (last_symbol_index + 1 >= info->symtab_size)
 	{
 	  if (mapping_type == MAP_DATA0)
@@ -1096,7 +1097,7 @@ print_insn_nds32 (bfd_vma pc, disassemble_info *info)
 	size = (pc & 1) ? 1 : 2;
 
       /* Read bytes from BFD.  */
-      info->read_memory_func (pc, (bfd_byte *) buf_data, size, info);
+      info->read_memory_func (pc, buf_data, size, info);
       given = 0;
       given1 = 0;
       /* Start assembling data.  */
@@ -1153,16 +1154,20 @@ print_insn_nds32 (bfd_vma pc, disassemble_info *info)
       return size;
     }
 
-  status = info->read_memory_func (pc, (bfd_byte *) buf, 4, info);
+  size = 4;
+  status = info->read_memory_func (pc, buf, 4, info);
   if (status)
     {
       /* For the last 16-bit instruction.  */
-      status = info->read_memory_func (pc, (bfd_byte *) buf, 2, info);
+      size = 2;
+      status = info->read_memory_func (pc, buf, 2, info);
       if (status)
 	{
-	  (*info->memory_error_func)(status, pc, info);
+	  (*info->memory_error_func) (status, pc, info);
 	  return -1;
 	}
+      buf[2] = 0;
+      buf[3] = 0;
     }
 
   insn = bfd_getb32 (buf);
@@ -1174,11 +1179,12 @@ print_insn_nds32 (bfd_vma pc, disassemble_info *info)
     }
 
   /* 32-bit instructions.  */
+  if (size == 4)
+    print_insn32 (pc, info, insn, NDS32_PARSE_INSN32);
   else
-    {
-      print_insn32 (pc, info, insn, NDS32_PARSE_INSN32);
-      return 4;
-    }
+    info->fprintf_func (info->stream,
+			_("insufficient data to decode instruction"));
+  return 4;
 }
 
 /* Ignore disassembling unnecessary name.  */
-- 
1.8.3.1

