From 3c5dcbec06d52582a33bd142000fe41581d79d04 Mon Sep 17 00:00:00 2001
From: Leo Yan <leo.yan@linaro.org>
Date: Fri, 31 Dec 2021 13:32:00 +0800
Subject: [PATCH 04/21] perf arm-spe: Refactor arm_spe_get_events()

mainline inclusion
from mainline-v5.11-rc1
commit b65577baf482909225c79d8a6bad44d2a62751f4
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I4NGPV
CVE: NA

-------------------------------------------------

In function arm_spe_get_events(), the event packet's 'index' is assigned
as payload length, but the flow is not directive: it firstly gets the
packet length from the return value of arm_spe_get_payload(), the value
includes header length (1) and payload length:

  int ret = arm_spe_get_payload(buf, len, packet);

and then reduces header length from packet length, so finally get the
payload length:

  packet->index = ret - 1;

To simplify the code, this patch directly assigns payload length to
event packet's index; and at the end it calls arm_spe_get_payload() to
return the payload value.

Signed-off-by: Leo Yan <leo.yan@linaro.org>
Reviewed-by: Andre Przywara <andre.przywara@arm.com>
Link: https://lore.kernel.org/r/20201111071149.815-5-leo.yan@linaro.org
Signed-off-by: Arnaldo Carvalho de Melo <acme@redhat.com>
Signed-off-by: Wei Li <liwei391@huawei.com>
Reviewed-by: Yang Jihong <yangjihong1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c | 6 ++----
 1 file changed, 2 insertions(+), 4 deletions(-)

diff --git a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
index a8eb7be189ec..57904da89db1 100644
--- a/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
+++ b/tools/perf/util/arm-spe-decoder/arm-spe-pkt-decoder.c
@@ -136,8 +136,6 @@ static int arm_spe_get_timestamp(const unsigned char *buf, size_t len,
 static int arm_spe_get_events(const unsigned char *buf, size_t len,
 			      struct arm_spe_pkt *packet)
 {
-	int ret = arm_spe_get_payload(buf, len, packet);
-
 	packet->type = ARM_SPE_EVENTS;
 
 	/* we use index to identify Events with a less number of
@@ -145,9 +143,9 @@ static int arm_spe_get_events(const unsigned char *buf, size_t len,
 	 * LLC-REFILL, and REMOTE-ACCESS events are identified if
 	 * index > 1.
 	 */
-	packet->index = ret - 1;
+	packet->index = arm_spe_payload_len(buf[0]);
 
-	return ret;
+	return arm_spe_get_payload(buf, len, packet);
 }
 
 static int arm_spe_get_data_source(const unsigned char *buf, size_t len,
-- 
2.27.0

