From 16c054f4640b9f7c21bb784ac54e1ea32ac65df0 Mon Sep 17 00:00:00 2001
From: Shaokun Zhang <zhangshaokun@hisilicon.com>
Date: Fri, 30 Jul 2021 15:44:08 +0800
Subject: [PATCH 19/55] drivers/perf: hisi: Add support for HiSilicon SLLC PMU
 driver

mainline inclusion
from mainline-v5.12-rc3
commit 3bf30882c3c7b6e376d9d6d04082c9aa2d2ac30a
category: feature
bugzilla: 175148
CVE: NA
Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=3bf30882c3c7b6e376d9d6d04082c9aa2d2ac30a

------------------------------------------------------------------------

HiSilicon's Hip09 is comprised by multi-dies that can be connected by SLLC
module (Skyros Link Layer Controller), its has separate PMU registers which
the driver can program it freely and interrupt is supported to handle
counter overflow. Let's support its driver under the framework of HiSilicon
uncore PMU driver.

SLLC PMU supports the following filter functions:
* tracetag_en: allows user to count data according to tt_req or
tt_core set in L3C PMU.

* srcid_cmd & srcid_msk: allows user to filter statistics that come from
specific CCL/ICL by configuration source ID.

* tgtid_hi & tgtid_lo: it also supports event statistics that these
operations will go to the CCL/ICL by configuration target ID or
target ID range. It's the same as source ID with 11-bit width in
the SoC. More introduction is added in documentation:
Documentation/admin-guide/perf/hisi-pmu.rst

Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Will Deacon <will@kernel.org>
Cc: John Garry <john.garry@huawei.com>
Cc: Jonathan Cameron <Jonathan.Cameron@huawei.com>
Reviewed-by: John Garry <john.garry@huawei.com>
Co-developed-by: Qi Liu <liuqi115@huawei.com>
Signed-off-by: Qi Liu <liuqi115@huawei.com>
Signed-off-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Link: https://lore.kernel.org/r/1615186237-22263-8-git-send-email-zhangshaokun@hisilicon.com
Signed-off-by: Will Deacon <will@kernel.org>
Reviewed-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>

 Conflicts:
	drivers/perf/hisilicon/Makefile
---
 drivers/perf/hisilicon/Makefile               |   4 +-
 drivers/perf/hisilicon/hisi_uncore_sllc_pmu.c | 530 ++++++++++++++++++
 include/linux/cpuhotplug.h                    |   1 +
 3 files changed, 534 insertions(+), 1 deletion(-)
 create mode 100644 drivers/perf/hisilicon/hisi_uncore_sllc_pmu.c

diff --git a/drivers/perf/hisilicon/Makefile b/drivers/perf/hisilicon/Makefile
index 2621d51ae87a..6600a9d45dd8 100644
--- a/drivers/perf/hisilicon/Makefile
+++ b/drivers/perf/hisilicon/Makefile
@@ -1 +1,3 @@
-obj-$(CONFIG_HISI_PMU) += hisi_uncore_pmu.o hisi_uncore_l3c_pmu.o hisi_uncore_hha_pmu.o hisi_uncore_ddrc_pmu.o
+# SPDX-License-Identifier: GPL-2.0-only
+obj-$(CONFIG_HISI_PMU) += hisi_uncore_pmu.o hisi_uncore_l3c_pmu.o \
+			  hisi_uncore_hha_pmu.o hisi_uncore_ddrc_pmu.o hisi_uncore_sllc_pmu.o
diff --git a/drivers/perf/hisilicon/hisi_uncore_sllc_pmu.c b/drivers/perf/hisilicon/hisi_uncore_sllc_pmu.c
new file mode 100644
index 000000000000..46be312fa126
--- /dev/null
+++ b/drivers/perf/hisilicon/hisi_uncore_sllc_pmu.c
@@ -0,0 +1,530 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * HiSilicon SLLC uncore Hardware event counters support
+ *
+ * Copyright (C) 2020 Hisilicon Limited
+ * Author: Shaokun Zhang <zhangshaokun@hisilicon.com>
+ *
+ * This code is based on the uncore PMUs like arm-cci and arm-ccn.
+ */
+#include <linux/acpi.h>
+#include <linux/cpuhotplug.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/list.h>
+#include <linux/smp.h>
+
+#include "hisi_uncore_pmu.h"
+
+/* SLLC register definition */
+#define SLLC_INT_MASK			0x0814
+#define SLLC_INT_STATUS			0x0818
+#define SLLC_INT_CLEAR			0x081c
+#define SLLC_PERF_CTRL			0x1c00
+#define SLLC_SRCID_CTRL			0x1c04
+#define SLLC_TGTID_CTRL			0x1c08
+#define SLLC_EVENT_CTRL			0x1c14
+#define SLLC_EVENT_TYPE0		0x1c18
+#define SLLC_VERSION			0x1cf0
+#define SLLC_EVENT_CNT0_L		0x1d00
+
+#define SLLC_EVTYPE_MASK		0xff
+#define SLLC_PERF_CTRL_EN		BIT(0)
+#define SLLC_FILT_EN			BIT(1)
+#define SLLC_TRACETAG_EN		BIT(2)
+#define SLLC_SRCID_EN			BIT(4)
+#define SLLC_SRCID_NONE			0x0
+#define SLLC_TGTID_EN			BIT(5)
+#define SLLC_TGTID_NONE			0x0
+#define SLLC_TGTID_MIN_SHIFT		1
+#define SLLC_TGTID_MAX_SHIFT		12
+#define SLLC_SRCID_CMD_SHIFT		1
+#define SLLC_SRCID_MSK_SHIFT		12
+#define SLLC_NR_EVENTS			0x80
+
+HISI_PMU_EVENT_ATTR_EXTRACTOR(tgtid_min, config1, 10, 0);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(tgtid_max, config1, 21, 11);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(srcid_cmd, config1, 32, 22);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(srcid_msk, config1, 43, 33);
+HISI_PMU_EVENT_ATTR_EXTRACTOR(tracetag_en, config1, 44, 44);
+
+static bool tgtid_is_valid(u32 max, u32 min)
+{
+	return max > 0 && max >= min;
+}
+
+static void hisi_sllc_pmu_enable_tracetag(struct perf_event *event)
+{
+	struct hisi_pmu *sllc_pmu = to_hisi_pmu(event->pmu);
+	u32 tt_en = hisi_get_tracetag_en(event);
+
+	if (tt_en) {
+		u32 val;
+
+		val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+		val |= SLLC_TRACETAG_EN | SLLC_FILT_EN;
+		writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+	}
+}
+
+static void hisi_sllc_pmu_disable_tracetag(struct perf_event *event)
+{
+	struct hisi_pmu *sllc_pmu = to_hisi_pmu(event->pmu);
+	u32 tt_en = hisi_get_tracetag_en(event);
+
+	if (tt_en) {
+		u32 val;
+
+		val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+		val &= ~(SLLC_TRACETAG_EN | SLLC_FILT_EN);
+		writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+	}
+}
+
+static void hisi_sllc_pmu_config_tgtid(struct perf_event *event)
+{
+	struct hisi_pmu *sllc_pmu = to_hisi_pmu(event->pmu);
+	u32 min = hisi_get_tgtid_min(event);
+	u32 max = hisi_get_tgtid_max(event);
+
+	if (tgtid_is_valid(max, min)) {
+		u32 val = (max << SLLC_TGTID_MAX_SHIFT) | (min << SLLC_TGTID_MIN_SHIFT);
+
+		writel(val, sllc_pmu->base + SLLC_TGTID_CTRL);
+		/* Enable the tgtid */
+		val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+		val |= SLLC_TGTID_EN | SLLC_FILT_EN;
+		writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+	}
+}
+
+static void hisi_sllc_pmu_clear_tgtid(struct perf_event *event)
+{
+	struct hisi_pmu *sllc_pmu = to_hisi_pmu(event->pmu);
+	u32 min = hisi_get_tgtid_min(event);
+	u32 max = hisi_get_tgtid_max(event);
+
+	if (tgtid_is_valid(max, min)) {
+		u32 val;
+
+		writel(SLLC_TGTID_NONE, sllc_pmu->base + SLLC_TGTID_CTRL);
+		/* Disable the tgtid */
+		val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+		val &= ~(SLLC_TGTID_EN | SLLC_FILT_EN);
+		writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+	}
+}
+
+static void hisi_sllc_pmu_config_srcid(struct perf_event *event)
+{
+	struct hisi_pmu *sllc_pmu = to_hisi_pmu(event->pmu);
+	u32 cmd = hisi_get_srcid_cmd(event);
+
+	if (cmd) {
+		u32 val, msk;
+
+		msk = hisi_get_srcid_msk(event);
+		val = (cmd << SLLC_SRCID_CMD_SHIFT) | (msk << SLLC_SRCID_MSK_SHIFT);
+		writel(val, sllc_pmu->base + SLLC_SRCID_CTRL);
+		/* Enable the srcid */
+		val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+		val |= SLLC_SRCID_EN | SLLC_FILT_EN;
+		writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+	}
+}
+
+static void hisi_sllc_pmu_clear_srcid(struct perf_event *event)
+{
+	struct hisi_pmu *sllc_pmu = to_hisi_pmu(event->pmu);
+	u32 cmd = hisi_get_srcid_cmd(event);
+
+	if (cmd) {
+		u32 val;
+
+		writel(SLLC_SRCID_NONE, sllc_pmu->base + SLLC_SRCID_CTRL);
+		/* Disable the srcid */
+		val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+		val &= ~(SLLC_SRCID_EN | SLLC_FILT_EN);
+		writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+	}
+}
+
+static void hisi_sllc_pmu_enable_filter(struct perf_event *event)
+{
+	if (event->attr.config1 != 0x0) {
+		hisi_sllc_pmu_enable_tracetag(event);
+		hisi_sllc_pmu_config_srcid(event);
+		hisi_sllc_pmu_config_tgtid(event);
+	}
+}
+
+static void hisi_sllc_pmu_clear_filter(struct perf_event *event)
+{
+	if (event->attr.config1 != 0x0) {
+		hisi_sllc_pmu_disable_tracetag(event);
+		hisi_sllc_pmu_clear_srcid(event);
+		hisi_sllc_pmu_clear_tgtid(event);
+	}
+}
+
+static u32 hisi_sllc_pmu_get_counter_offset(int idx)
+{
+	return (SLLC_EVENT_CNT0_L + idx * 8);
+}
+
+static u64 hisi_sllc_pmu_read_counter(struct hisi_pmu *sllc_pmu,
+				      struct hw_perf_event *hwc)
+{
+	return readq(sllc_pmu->base +
+		     hisi_sllc_pmu_get_counter_offset(hwc->idx));
+}
+
+static void hisi_sllc_pmu_write_counter(struct hisi_pmu *sllc_pmu,
+					struct hw_perf_event *hwc, u64 val)
+{
+	writeq(val, sllc_pmu->base +
+	       hisi_sllc_pmu_get_counter_offset(hwc->idx));
+}
+
+static void hisi_sllc_pmu_write_evtype(struct hisi_pmu *sllc_pmu, int idx,
+				       u32 type)
+{
+	u32 reg, reg_idx, shift, val;
+
+	/*
+	 * Select the appropriate event select register(SLLC_EVENT_TYPE0/1).
+	 * There are 2 event select registers for the 8 hardware counters.
+	 * Event code is 8-bits and for the former 4 hardware counters,
+	 * SLLC_EVENT_TYPE0 is chosen. For the latter 4 hardware counters,
+	 * SLLC_EVENT_TYPE1 is chosen.
+	 */
+	reg = SLLC_EVENT_TYPE0 + (idx / 4) * 4;
+	reg_idx = idx % 4;
+	shift = 8 * reg_idx;
+
+	/* Write event code to SLLC_EVENT_TYPEx Register */
+	val = readl(sllc_pmu->base + reg);
+	val &= ~(SLLC_EVTYPE_MASK << shift);
+	val |= (type << shift);
+	writel(val, sllc_pmu->base + reg);
+}
+
+static void hisi_sllc_pmu_start_counters(struct hisi_pmu *sllc_pmu)
+{
+	u32 val;
+
+	val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+	val |= SLLC_PERF_CTRL_EN;
+	writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+}
+
+static void hisi_sllc_pmu_stop_counters(struct hisi_pmu *sllc_pmu)
+{
+	u32 val;
+
+	val = readl(sllc_pmu->base + SLLC_PERF_CTRL);
+	val &= ~(SLLC_PERF_CTRL_EN);
+	writel(val, sllc_pmu->base + SLLC_PERF_CTRL);
+}
+
+static void hisi_sllc_pmu_enable_counter(struct hisi_pmu *sllc_pmu,
+					 struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	val = readl(sllc_pmu->base + SLLC_EVENT_CTRL);
+	val |= 1 << hwc->idx;
+	writel(val, sllc_pmu->base + SLLC_EVENT_CTRL);
+}
+
+static void hisi_sllc_pmu_disable_counter(struct hisi_pmu *sllc_pmu,
+					  struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	val = readl(sllc_pmu->base + SLLC_EVENT_CTRL);
+	val &= ~(1 << hwc->idx);
+	writel(val, sllc_pmu->base + SLLC_EVENT_CTRL);
+}
+
+static void hisi_sllc_pmu_enable_counter_int(struct hisi_pmu *sllc_pmu,
+					     struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	val = readl(sllc_pmu->base + SLLC_INT_MASK);
+	/* Write 0 to enable interrupt */
+	val &= ~(1 << hwc->idx);
+	writel(val, sllc_pmu->base + SLLC_INT_MASK);
+}
+
+static void hisi_sllc_pmu_disable_counter_int(struct hisi_pmu *sllc_pmu,
+					      struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	val = readl(sllc_pmu->base + SLLC_INT_MASK);
+	/* Write 1 to mask interrupt */
+	val |= 1 << hwc->idx;
+	writel(val, sllc_pmu->base + SLLC_INT_MASK);
+}
+
+static u32 hisi_sllc_pmu_get_int_status(struct hisi_pmu *sllc_pmu)
+{
+	return readl(sllc_pmu->base + SLLC_INT_STATUS);
+}
+
+static void hisi_sllc_pmu_clear_int_status(struct hisi_pmu *sllc_pmu, int idx)
+{
+	writel(1 << idx, sllc_pmu->base + SLLC_INT_CLEAR);
+}
+
+static const struct acpi_device_id hisi_sllc_pmu_acpi_match[] = {
+	{ "HISI0263", },
+	{}
+};
+MODULE_DEVICE_TABLE(acpi, hisi_sllc_pmu_acpi_match);
+
+static int hisi_sllc_pmu_init_data(struct platform_device *pdev,
+				   struct hisi_pmu *sllc_pmu)
+{
+	/*
+	 * Use the SCCL_ID and the index ID to identify the SLLC PMU,
+	 * while SCCL_ID is from MPIDR_EL1 by CPU.
+	 */
+	if (device_property_read_u32(&pdev->dev, "hisilicon,scl-id",
+				     &sllc_pmu->sccl_id)) {
+		dev_err(&pdev->dev, "Cannot read sccl-id!\n");
+		return -EINVAL;
+	}
+
+	if (device_property_read_u32(&pdev->dev, "hisilicon,idx-id",
+				     &sllc_pmu->index_id)) {
+		dev_err(&pdev->dev, "Cannot read idx-id!\n");
+		return -EINVAL;
+	}
+
+	/* SLLC PMUs only share the same SCCL */
+	sllc_pmu->ccl_id = -1;
+
+	sllc_pmu->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(sllc_pmu->base)) {
+		dev_err(&pdev->dev, "ioremap failed for sllc_pmu resource.\n");
+		return PTR_ERR(sllc_pmu->base);
+	}
+
+	sllc_pmu->identifier = readl(sllc_pmu->base + SLLC_VERSION);
+
+	return 0;
+}
+
+static struct attribute *hisi_sllc_pmu_v2_format_attr[] = {
+	HISI_PMU_FORMAT_ATTR(event, "config:0-7"),
+	HISI_PMU_FORMAT_ATTR(tgtid_min, "config1:0-10"),
+	HISI_PMU_FORMAT_ATTR(tgtid_max, "config1:11-21"),
+	HISI_PMU_FORMAT_ATTR(srcid_cmd, "config1:22-32"),
+	HISI_PMU_FORMAT_ATTR(srcid_msk, "config1:33-43"),
+	HISI_PMU_FORMAT_ATTR(tracetag_en, "config1:44"),
+	NULL
+};
+
+static const struct attribute_group hisi_sllc_pmu_v2_format_group = {
+	.name = "format",
+	.attrs = hisi_sllc_pmu_v2_format_attr,
+};
+
+static struct attribute *hisi_sllc_pmu_v2_events_attr[] = {
+	HISI_PMU_EVENT_ATTR(rx_req,             0x30),
+	HISI_PMU_EVENT_ATTR(rx_data,            0x31),
+	HISI_PMU_EVENT_ATTR(tx_req,             0x34),
+	HISI_PMU_EVENT_ATTR(tx_data,            0x35),
+	HISI_PMU_EVENT_ATTR(cycles,             0x09),
+	NULL
+};
+
+static const struct attribute_group hisi_sllc_pmu_v2_events_group = {
+	.name = "events",
+	.attrs = hisi_sllc_pmu_v2_events_attr,
+};
+
+static DEVICE_ATTR(cpumask, 0444, hisi_cpumask_sysfs_show, NULL);
+
+static struct attribute *hisi_sllc_pmu_cpumask_attrs[] = {
+	&dev_attr_cpumask.attr,
+	NULL
+};
+
+static const struct attribute_group hisi_sllc_pmu_cpumask_attr_group = {
+	.attrs = hisi_sllc_pmu_cpumask_attrs,
+};
+
+static struct device_attribute hisi_sllc_pmu_identifier_attr =
+	__ATTR(identifier, 0444, hisi_uncore_pmu_identifier_attr_show, NULL);
+
+static struct attribute *hisi_sllc_pmu_identifier_attrs[] = {
+	&hisi_sllc_pmu_identifier_attr.attr,
+	NULL
+};
+
+static struct attribute_group hisi_sllc_pmu_identifier_group = {
+	.attrs = hisi_sllc_pmu_identifier_attrs,
+};
+
+static const struct attribute_group *hisi_sllc_pmu_v2_attr_groups[] = {
+	&hisi_sllc_pmu_v2_format_group,
+	&hisi_sllc_pmu_v2_events_group,
+	&hisi_sllc_pmu_cpumask_attr_group,
+	&hisi_sllc_pmu_identifier_group,
+	NULL
+};
+
+static const struct hisi_uncore_ops hisi_uncore_sllc_ops = {
+	.write_evtype		= hisi_sllc_pmu_write_evtype,
+	.get_event_idx		= hisi_uncore_pmu_get_event_idx,
+	.start_counters		= hisi_sllc_pmu_start_counters,
+	.stop_counters		= hisi_sllc_pmu_stop_counters,
+	.enable_counter		= hisi_sllc_pmu_enable_counter,
+	.disable_counter	= hisi_sllc_pmu_disable_counter,
+	.enable_counter_int	= hisi_sllc_pmu_enable_counter_int,
+	.disable_counter_int	= hisi_sllc_pmu_disable_counter_int,
+	.write_counter		= hisi_sllc_pmu_write_counter,
+	.read_counter		= hisi_sllc_pmu_read_counter,
+	.get_int_status		= hisi_sllc_pmu_get_int_status,
+	.clear_int_status	= hisi_sllc_pmu_clear_int_status,
+	.enable_filter		= hisi_sllc_pmu_enable_filter,
+	.disable_filter		= hisi_sllc_pmu_clear_filter,
+};
+
+static int hisi_sllc_pmu_dev_probe(struct platform_device *pdev,
+				   struct hisi_pmu *sllc_pmu)
+{
+	int ret;
+
+	ret = hisi_sllc_pmu_init_data(pdev, sllc_pmu);
+	if (ret)
+		return ret;
+
+	ret = hisi_uncore_pmu_init_irq(sllc_pmu, pdev);
+	if (ret)
+		return ret;
+
+	sllc_pmu->pmu_events.attr_groups = hisi_sllc_pmu_v2_attr_groups;
+	sllc_pmu->ops = &hisi_uncore_sllc_ops;
+	sllc_pmu->check_event = SLLC_NR_EVENTS;
+	sllc_pmu->counter_bits = 64;
+	sllc_pmu->num_counters = 8;
+	sllc_pmu->dev = &pdev->dev;
+	sllc_pmu->on_cpu = -1;
+
+	return 0;
+}
+
+static int hisi_sllc_pmu_probe(struct platform_device *pdev)
+{
+	struct hisi_pmu *sllc_pmu;
+	char *name;
+	int ret;
+
+	sllc_pmu = devm_kzalloc(&pdev->dev, sizeof(*sllc_pmu), GFP_KERNEL);
+	if (!sllc_pmu)
+		return -ENOMEM;
+
+	ret = hisi_sllc_pmu_dev_probe(pdev, sllc_pmu);
+	if (ret)
+		return ret;
+
+	name = devm_kasprintf(&pdev->dev, GFP_KERNEL, "hisi_sccl%u_sllc%u",
+			      sllc_pmu->sccl_id, sllc_pmu->index_id);
+	if (!name)
+		return -ENOMEM;
+
+	ret = cpuhp_state_add_instance(CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE,
+				       &sllc_pmu->node);
+	if (ret) {
+		dev_err(&pdev->dev, "Error %d registering hotplug\n", ret);
+		return ret;
+	}
+
+	sllc_pmu->pmu = (struct pmu) {
+		.module		= THIS_MODULE,
+		.task_ctx_nr	= perf_invalid_context,
+		.event_init	= hisi_uncore_pmu_event_init,
+		.pmu_enable	= hisi_uncore_pmu_enable,
+		.pmu_disable	= hisi_uncore_pmu_disable,
+		.add		= hisi_uncore_pmu_add,
+		.del		= hisi_uncore_pmu_del,
+		.start		= hisi_uncore_pmu_start,
+		.stop		= hisi_uncore_pmu_stop,
+		.read		= hisi_uncore_pmu_read,
+		.attr_groups    = sllc_pmu->pmu_events.attr_groups,
+		.capabilities	= PERF_PMU_CAP_NO_EXCLUDE,
+	};
+
+	ret = perf_pmu_register(&sllc_pmu->pmu, name, -1);
+	if (ret) {
+		dev_err(sllc_pmu->dev, "PMU register failed, ret = %d\n", ret);
+		cpuhp_state_remove_instance(CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE,
+					    &sllc_pmu->node);
+		irq_set_affinity_hint(sllc_pmu->irq, NULL);
+		return ret;
+	}
+
+	platform_set_drvdata(pdev, sllc_pmu);
+
+	return ret;
+}
+
+static int hisi_sllc_pmu_remove(struct platform_device *pdev)
+{
+	struct hisi_pmu *sllc_pmu = platform_get_drvdata(pdev);
+
+	perf_pmu_unregister(&sllc_pmu->pmu);
+	cpuhp_state_remove_instance_nocalls(CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE,
+					    &sllc_pmu->node);
+	irq_set_affinity_hint(sllc_pmu->irq, NULL);
+
+	return 0;
+}
+
+static struct platform_driver hisi_sllc_pmu_driver = {
+	.driver = {
+		.name = "hisi_sllc_pmu",
+		.acpi_match_table = hisi_sllc_pmu_acpi_match,
+		.suppress_bind_attrs = true,
+	},
+	.probe = hisi_sllc_pmu_probe,
+	.remove = hisi_sllc_pmu_remove,
+};
+
+static int __init hisi_sllc_pmu_module_init(void)
+{
+	int ret;
+
+	ret = cpuhp_setup_state_multi(CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE,
+				      "AP_PERF_ARM_HISI_SLLC_ONLINE",
+				      hisi_uncore_pmu_online_cpu,
+				      hisi_uncore_pmu_offline_cpu);
+	if (ret) {
+		pr_err("SLLC PMU: cpuhp state setup failed, ret = %d\n", ret);
+		return ret;
+	}
+
+	ret = platform_driver_register(&hisi_sllc_pmu_driver);
+	if (ret)
+		cpuhp_remove_multi_state(CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE);
+
+	return ret;
+}
+module_init(hisi_sllc_pmu_module_init);
+
+static void __exit hisi_sllc_pmu_module_exit(void)
+{
+	platform_driver_unregister(&hisi_sllc_pmu_driver);
+	cpuhp_remove_multi_state(CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE);
+}
+module_exit(hisi_sllc_pmu_module_exit);
+
+MODULE_DESCRIPTION("HiSilicon SLLC uncore PMU driver");
+MODULE_LICENSE("GPL v2");
+MODULE_AUTHOR("Shaokun Zhang <zhangshaokun@hisilicon.com>");
+MODULE_AUTHOR("Qi Liu <liuqi115@huawei.com>");
diff --git a/include/linux/cpuhotplug.h b/include/linux/cpuhotplug.h
index d67c0035165c..b5c55a408a30 100644
--- a/include/linux/cpuhotplug.h
+++ b/include/linux/cpuhotplug.h
@@ -161,6 +161,7 @@ enum cpuhp_state {
 	CPUHP_AP_PERF_ARM_HISI_DDRC_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_HHA_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_L3_ONLINE,
+	CPUHP_AP_PERF_ARM_HISI_SLLC_ONLINE,
 	CPUHP_AP_PERF_ARM_L2X0_ONLINE,
 	CPUHP_AP_PERF_ARM_QCOM_L2_ONLINE,
 	CPUHP_AP_PERF_ARM_QCOM_L3_ONLINE,
-- 
2.27.0

