From 34861133469cfd5c5851f7f4ab05e3d3af1dd13a Mon Sep 17 00:00:00 2001
From: Shaokun Zhang <zhangshaokun@hisilicon.com>
Date: Fri, 30 Jul 2021 15:44:02 +0800
Subject: [PATCH 13/55] drivers/perf: hisi: Remove unnecessary check of counter
 index

mainline inclusion
from mainline-v5.12-rc3
commit 4e4cb8ca48bd68c00df67c10ff867016abb7391f
category: cleanup
bugzilla: 175148
CVE: NA
Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=4e4cb8ca48bd68c00df67c10ff867016abb7391f

------------------------------------------------------------------------

The sanity check for counter index has been done in the function
hisi_uncore_pmu_get_event_idx, so remove the redundant interface
hisi_uncore_pmu_counter_valid() and sanity check.

Cc: Mark Rutland <mark.rutland@arm.com>
Cc: Will Deacon <will@kernel.org>
Cc: John Garry <john.garry@huawei.com>
Cc: Jonathan Cameron <Jonathan.Cameron@huawei.com>
Co-developed-by: Qi Liu <liuqi115@huawei.com>
Signed-off-by: Qi Liu <liuqi115@huawei.com>
Signed-off-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Link: https://lore.kernel.org/r/1615186237-22263-2-git-send-email-zhangshaokun@hisilicon.com
Signed-off-by: Will Deacon <will@kernel.org>
Reviewed-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c | 20 +++----------------
 drivers/perf/hisilicon/hisi_uncore_hha_pmu.c  | 18 ++---------------
 drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c  | 18 ++---------------
 drivers/perf/hisilicon/hisi_uncore_pmu.c      | 11 ----------
 drivers/perf/hisilicon/hisi_uncore_pmu.h      |  1 -
 5 files changed, 7 insertions(+), 61 deletions(-)

diff --git a/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c b/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c
index a88c7d840d38..bcb2c2d66b7f 100644
--- a/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_ddrc_pmu.c
@@ -68,29 +68,15 @@ static u32 hisi_ddrc_pmu_get_counter_offset(int cntr_idx)
 static u64 hisi_ddrc_pmu_read_counter(struct hisi_pmu *ddrc_pmu,
 				      struct hw_perf_event *hwc)
 {
-	/* Use event code as counter index */
-	u32 idx = GET_DDRC_EVENTID(hwc);
-
-	if (!hisi_uncore_pmu_counter_valid(ddrc_pmu, idx)) {
-		dev_err(ddrc_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return 0;
-	}
-
-	return readl(ddrc_pmu->base + hisi_ddrc_pmu_get_counter_offset(idx));
+	return readl(ddrc_pmu->base +
+		     hisi_ddrc_pmu_get_counter_offset(hwc->idx));
 }
 
 static void hisi_ddrc_pmu_write_counter(struct hisi_pmu *ddrc_pmu,
 					struct hw_perf_event *hwc, u64 val)
 {
-	u32 idx = GET_DDRC_EVENTID(hwc);
-
-	if (!hisi_uncore_pmu_counter_valid(ddrc_pmu, idx)) {
-		dev_err(ddrc_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return;
-	}
-
 	writel((u32)val,
-	       ddrc_pmu->base + hisi_ddrc_pmu_get_counter_offset(idx));
+	       ddrc_pmu->base + hisi_ddrc_pmu_get_counter_offset(hwc->idx));
 }
 
 /*
diff --git a/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c b/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c
index 1e0138bbe6e7..de1766342b4e 100644
--- a/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_hha_pmu.c
@@ -54,29 +54,15 @@ static u32 hisi_hha_pmu_get_counter_offset(u32 cntr_idx)
 static u64 hisi_hha_pmu_read_counter(struct hisi_pmu *hha_pmu,
 				     struct hw_perf_event *hwc)
 {
-	u32 idx = hwc->idx;
-
-	if (!hisi_uncore_pmu_counter_valid(hha_pmu, idx)) {
-		dev_err(hha_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return 0;
-	}
-
 	/* Read 64 bits and like L3C, top 16 bits are RAZ */
-	return readq(hha_pmu->base + hisi_hha_pmu_get_counter_offset(idx));
+	return readq(hha_pmu->base + hisi_hha_pmu_get_counter_offset(hwc->idx));
 }
 
 static void hisi_hha_pmu_write_counter(struct hisi_pmu *hha_pmu,
 				       struct hw_perf_event *hwc, u64 val)
 {
-	u32 idx = hwc->idx;
-
-	if (!hisi_uncore_pmu_counter_valid(hha_pmu, idx)) {
-		dev_err(hha_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return;
-	}
-
 	/* Write 64 bits and like L3C, top 16 bits are WI */
-	writeq(val, hha_pmu->base + hisi_hha_pmu_get_counter_offset(idx));
+	writeq(val, hha_pmu->base + hisi_hha_pmu_get_counter_offset(hwc->idx));
 }
 
 static void hisi_hha_pmu_write_evtype(struct hisi_pmu *hha_pmu, int idx,
diff --git a/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c b/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c
index 1707ae551ece..c4afeaaaa3a4 100644
--- a/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_l3c_pmu.c
@@ -53,29 +53,15 @@ static u32 hisi_l3c_pmu_get_counter_offset(u32 cntr_idx)
 static u64 hisi_l3c_pmu_read_counter(struct hisi_pmu *l3c_pmu,
 				     struct hw_perf_event *hwc)
 {
-	u32 idx = hwc->idx;
-
-	if (!hisi_uncore_pmu_counter_valid(l3c_pmu, idx)) {
-		dev_err(l3c_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return 0;
-	}
-
 	/* Read 64-bits and the upper 16 bits are RAZ */
-	return readq(l3c_pmu->base + hisi_l3c_pmu_get_counter_offset(idx));
+	return readq(l3c_pmu->base + hisi_l3c_pmu_get_counter_offset(hwc->idx));
 }
 
 static void hisi_l3c_pmu_write_counter(struct hisi_pmu *l3c_pmu,
 				       struct hw_perf_event *hwc, u64 val)
 {
-	u32 idx = hwc->idx;
-
-	if (!hisi_uncore_pmu_counter_valid(l3c_pmu, idx)) {
-		dev_err(l3c_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return;
-	}
-
 	/* Write 64-bits and the upper 16 bits are WI */
-	writeq(val, l3c_pmu->base + hisi_l3c_pmu_get_counter_offset(idx));
+	writeq(val, l3c_pmu->base + hisi_l3c_pmu_get_counter_offset(hwc->idx));
 }
 
 static void hisi_l3c_pmu_write_evtype(struct hisi_pmu *l3c_pmu, int idx,
diff --git a/drivers/perf/hisilicon/hisi_uncore_pmu.c b/drivers/perf/hisilicon/hisi_uncore_pmu.c
index f6a992da24bf..9ebdb76dd3a4 100644
--- a/drivers/perf/hisilicon/hisi_uncore_pmu.c
+++ b/drivers/perf/hisilicon/hisi_uncore_pmu.c
@@ -99,12 +99,6 @@ static bool hisi_validate_event_group(struct perf_event *event)
 	return counters <= hisi_pmu->num_counters;
 }
 
-int hisi_uncore_pmu_counter_valid(struct hisi_pmu *hisi_pmu, int idx)
-{
-	return idx >= 0 && idx < hisi_pmu->num_counters;
-}
-EXPORT_SYMBOL_GPL(hisi_uncore_pmu_counter_valid);
-
 int hisi_uncore_pmu_get_event_idx(struct perf_event *event)
 {
 	struct hisi_pmu *hisi_pmu = to_hisi_pmu(event->pmu);
@@ -134,11 +128,6 @@ EXPORT_SYMBOL_GPL(hisi_uncore_pmu_identifier_attr_show);
 
 static void hisi_uncore_pmu_clear_event_idx(struct hisi_pmu *hisi_pmu, int idx)
 {
-	if (!hisi_uncore_pmu_counter_valid(hisi_pmu, idx)) {
-		dev_err(hisi_pmu->dev, "Unsupported event index:%d!\n", idx);
-		return;
-	}
-
 	clear_bit(idx, hisi_pmu->pmu_events.used_mask);
 }
 
diff --git a/drivers/perf/hisilicon/hisi_uncore_pmu.h b/drivers/perf/hisilicon/hisi_uncore_pmu.h
index 098a8f6dc7ee..d71a6c86b282 100644
--- a/drivers/perf/hisilicon/hisi_uncore_pmu.h
+++ b/drivers/perf/hisilicon/hisi_uncore_pmu.h
@@ -81,7 +81,6 @@ struct hisi_pmu {
 	u32 identifier;
 };
 
-int hisi_uncore_pmu_counter_valid(struct hisi_pmu *hisi_pmu, int idx);
 int hisi_uncore_pmu_get_event_idx(struct perf_event *event);
 void hisi_uncore_pmu_read(struct perf_event *event);
 int hisi_uncore_pmu_add(struct perf_event *event, int flags);
-- 
2.27.0

