From a75b20496157f6605843bf6399c7d082ec2a37b2 Mon Sep 17 00:00:00 2001
From: Qi Liu <liuqi115@huawei.com>
Date: Tue, 9 Aug 2022 23:06:43 +0800
Subject: [PATCH 32/55] drivers/perf: hisi: Add Support for CPA PMU

mainline inclusion
from mainline-v5.19-rc1
commit 6b79738b6ed91a2d0fe958819469eeedac3bca81
category: feature
bugzilla: https://gitee.com/openeuler/kernel/issues/I5AZ87
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=6b79738b6ed9

--------------------------------------------------------------------------

On HiSilicon Hip09 platform, there is a CPA (Coherency Protocol Agent) on
each SICL (Super IO Cluster) which implements packet format translation,
route parsing and traffic statistics.

CPA PMU has 8 PMU counters and interrupt is supported to handle counter
overflow. Let's support its driver under the framework of HiSilicon PMU
driver.

Signed-off-by: Qi Liu <liuqi115@huawei.com>
Reviewed-by: John Garry <john.garry@huawei.com>
Reviewed-by: Shaokun Zhang <zhangshaokun@hisilicon.com>
Link: https://lore.kernel.org/r/20220415102352.6665-3-liuqi115@huawei.com
Signed-off-by: Will Deacon <will@kernel.org>
Signed-off-by: Wangming Shao <shaowangming@h-partners.com>
Reviewed-by: Junhao He <hejunhao3@huawei.com>
Reviewed-by: Yang Jihong <yangjihong1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: hongrongxuan <hongrongxuan@huawei.com>
---
 drivers/perf/hisilicon/Makefile              |   2 +-
 drivers/perf/hisilicon/hisi_uncore_cpa_pmu.c | 409 +++++++++++++++++++
 include/linux/cpuhotplug.h                   |   3 +
 3 files changed, 413 insertions(+), 1 deletion(-)
 create mode 100644 drivers/perf/hisilicon/hisi_uncore_cpa_pmu.c

diff --git a/drivers/perf/hisilicon/Makefile b/drivers/perf/hisilicon/Makefile
index ad0e8110f373..a3522abb3975 100644
--- a/drivers/perf/hisilicon/Makefile
+++ b/drivers/perf/hisilicon/Makefile
@@ -1,7 +1,7 @@
 # SPDX-License-Identifier: GPL-2.0-only
 obj-$(CONFIG_HISI_PMU) += hisi_uncore_pmu.o hisi_uncore_l3c_pmu.o \
 			  hisi_uncore_hha_pmu.o hisi_uncore_ddrc_pmu.o hisi_uncore_sllc_pmu.o \
-			  hisi_uncore_pa_pmu.o \
+			  hisi_uncore_pa_pmu.o hisi_uncore_cpa_pmu.o \
 			  hisi_uncore_l3t_pmu.o \
 			  hisi_uncore_lpddrc_pmu.o
 
diff --git a/drivers/perf/hisilicon/hisi_uncore_cpa_pmu.c b/drivers/perf/hisilicon/hisi_uncore_cpa_pmu.c
new file mode 100644
index 000000000000..a9bb73f76be4
--- /dev/null
+++ b/drivers/perf/hisilicon/hisi_uncore_cpa_pmu.c
@@ -0,0 +1,409 @@
+// SPDX-License-Identifier: GPL-2.0-only
+/*
+ * HiSilicon SoC CPA(Coherency Protocol Agent) hardware event counters support
+ *
+ * Copyright (C) 2022 HiSilicon Limited
+ * Author: Qi Liu <liuqi115@huawei.com>
+ *
+ * This code is based on the uncore PMUs like arm-cci and arm-ccn.
+ */
+
+#define pr_fmt(fmt) "cpa pmu: " fmt
+#include <linux/acpi.h>
+#include <linux/bug.h>
+#include <linux/cpuhotplug.h>
+#include <linux/interrupt.h>
+#include <linux/irq.h>
+#include <linux/list.h>
+#include <linux/smp.h>
+
+#include "hisi_uncore_pmu.h"
+
+/* CPA register definition */
+#define CPA_PERF_CTRL		0x1c00
+#define CPA_EVENT_CTRL		0x1c04
+#define CPA_INT_MASK		0x1c70
+#define CPA_INT_STATUS		0x1c78
+#define CPA_INT_CLEAR		0x1c7c
+#define CPA_EVENT_TYPE0		0x1c80
+#define CPA_VERSION		0x1cf0
+#define CPA_CNT0_LOWER		0x1d00
+#define CPA_CFG_REG		0x0534
+
+/* CPA operation command */
+#define CPA_PERF_CTRL_EN	BIT_ULL(0)
+#define CPA_EVTYPE_MASK		0xffUL
+#define CPA_PM_CTRL		BIT_ULL(9)
+
+/* CPA has 8-counters */
+#define CPA_NR_COUNTERS		0x8
+#define CPA_COUNTER_BITS	64
+#define CPA_NR_EVENTS		0xff
+#define CPA_REG_OFFSET		0x8
+
+static u32 hisi_cpa_pmu_get_counter_offset(int idx)
+{
+	return (CPA_CNT0_LOWER + idx * CPA_REG_OFFSET);
+}
+
+static u64 hisi_cpa_pmu_read_counter(struct hisi_pmu *cpa_pmu,
+				     struct hw_perf_event *hwc)
+{
+	return readq(cpa_pmu->base + hisi_cpa_pmu_get_counter_offset(hwc->idx));
+}
+
+static void hisi_cpa_pmu_write_counter(struct hisi_pmu *cpa_pmu,
+				       struct hw_perf_event *hwc, u64 val)
+{
+	writeq(val, cpa_pmu->base + hisi_cpa_pmu_get_counter_offset(hwc->idx));
+}
+
+static void hisi_cpa_pmu_write_evtype(struct hisi_pmu *cpa_pmu, int idx,
+				      u32 type)
+{
+	u32 reg, reg_idx, shift, val;
+
+	/*
+	 * Select the appropriate event select register(CPA_EVENT_TYPE0/1).
+	 * There are 2 event select registers for the 8 hardware counters.
+	 * Event code is 8-bits and for the former 4 hardware counters,
+	 * CPA_EVENT_TYPE0 is chosen. For the latter 4 hardware counters,
+	 * CPA_EVENT_TYPE1 is chosen.
+	 */
+	reg = CPA_EVENT_TYPE0 + (idx / 4) * 4;
+	reg_idx = idx % 4;
+	shift = CPA_REG_OFFSET * reg_idx;
+
+	/* Write event code to CPA_EVENT_TYPEx Register */
+	val = readl(cpa_pmu->base + reg);
+	val &= ~(CPA_EVTYPE_MASK << shift);
+	val |= type << shift;
+	writel(val, cpa_pmu->base + reg);
+}
+
+static void hisi_cpa_pmu_start_counters(struct hisi_pmu *cpa_pmu)
+{
+	u32 val;
+
+	val = readl(cpa_pmu->base + CPA_PERF_CTRL);
+	val |= CPA_PERF_CTRL_EN;
+	writel(val, cpa_pmu->base + CPA_PERF_CTRL);
+}
+
+static void hisi_cpa_pmu_stop_counters(struct hisi_pmu *cpa_pmu)
+{
+	u32 val;
+
+	val = readl(cpa_pmu->base + CPA_PERF_CTRL);
+	val &= ~(CPA_PERF_CTRL_EN);
+	writel(val, cpa_pmu->base + CPA_PERF_CTRL);
+}
+
+static void hisi_cpa_pmu_disable_pm(struct hisi_pmu *cpa_pmu)
+{
+	u32 val;
+
+	val = readl(cpa_pmu->base + CPA_CFG_REG);
+	val |= CPA_PM_CTRL;
+	writel(val, cpa_pmu->base + CPA_CFG_REG);
+}
+
+static void hisi_cpa_pmu_enable_pm(struct hisi_pmu *cpa_pmu)
+{
+	u32 val;
+
+	val = readl(cpa_pmu->base + CPA_CFG_REG);
+	val &= ~(CPA_PM_CTRL);
+	writel(val, cpa_pmu->base + CPA_CFG_REG);
+}
+
+static void hisi_cpa_pmu_enable_counter(struct hisi_pmu *cpa_pmu,
+					struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Enable counter index in CPA_EVENT_CTRL register */
+	val = readl(cpa_pmu->base + CPA_EVENT_CTRL);
+	val |= 1 << hwc->idx;
+	writel(val, cpa_pmu->base + CPA_EVENT_CTRL);
+}
+
+static void hisi_cpa_pmu_disable_counter(struct hisi_pmu *cpa_pmu,
+					 struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Clear counter index in CPA_EVENT_CTRL register */
+	val = readl(cpa_pmu->base + CPA_EVENT_CTRL);
+	val &= ~(1UL << hwc->idx);
+	writel(val, cpa_pmu->base + CPA_EVENT_CTRL);
+}
+
+static void hisi_cpa_pmu_enable_counter_int(struct hisi_pmu *cpa_pmu,
+					    struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Write 0 to enable interrupt */
+	val = readl(cpa_pmu->base + CPA_INT_MASK);
+	val &= ~(1UL << hwc->idx);
+	writel(val, cpa_pmu->base + CPA_INT_MASK);
+}
+
+static void hisi_cpa_pmu_disable_counter_int(struct hisi_pmu *cpa_pmu,
+					     struct hw_perf_event *hwc)
+{
+	u32 val;
+
+	/* Write 1 to mask interrupt */
+	val = readl(cpa_pmu->base + CPA_INT_MASK);
+	val |= 1 << hwc->idx;
+	writel(val, cpa_pmu->base + CPA_INT_MASK);
+}
+
+static u32 hisi_cpa_pmu_get_int_status(struct hisi_pmu *cpa_pmu)
+{
+	return readl(cpa_pmu->base + CPA_INT_STATUS);
+}
+
+static void hisi_cpa_pmu_clear_int_status(struct hisi_pmu *cpa_pmu, int idx)
+{
+	writel(1 << idx, cpa_pmu->base + CPA_INT_CLEAR);
+}
+
+static const struct acpi_device_id hisi_cpa_pmu_acpi_match[] = {
+	{ "HISI0281", },
+	{}
+};
+MODULE_DEVICE_TABLE(acpi, hisi_cpa_pmu_acpi_match);
+
+static int hisi_cpa_pmu_init_data(struct platform_device *pdev,
+				  struct hisi_pmu *cpa_pmu)
+{
+	if (device_property_read_u32(&pdev->dev, "hisilicon,scl-id",
+				     &cpa_pmu->sicl_id)) {
+		dev_err(&pdev->dev, "Can not read sicl-id\n");
+		return -EINVAL;
+	}
+
+	if (device_property_read_u32(&pdev->dev, "hisilicon,idx-id",
+				     &cpa_pmu->index_id)) {
+		dev_err(&pdev->dev, "Cannot read idx-id\n");
+		return -EINVAL;
+	}
+
+	cpa_pmu->ccl_id = -1;
+	cpa_pmu->sccl_id = -1;
+	cpa_pmu->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(cpa_pmu->base))
+		return PTR_ERR(cpa_pmu->base);
+
+	cpa_pmu->identifier = readl(cpa_pmu->base + CPA_VERSION);
+
+	return 0;
+}
+
+static struct attribute *hisi_cpa_pmu_format_attr[] = {
+	HISI_PMU_FORMAT_ATTR(event, "config:0-15"),
+	NULL
+};
+
+static const struct attribute_group hisi_cpa_pmu_format_group = {
+	.name = "format",
+	.attrs = hisi_cpa_pmu_format_attr,
+};
+
+static struct attribute *hisi_cpa_pmu_events_attr[] = {
+	HISI_PMU_EVENT_ATTR(cpa_cycles,		0x00),
+	HISI_PMU_EVENT_ATTR(cpa_p1_wr_dat,	0x61),
+	HISI_PMU_EVENT_ATTR(cpa_p1_rd_dat,	0x62),
+	HISI_PMU_EVENT_ATTR(cpa_p0_wr_dat,	0xE1),
+	HISI_PMU_EVENT_ATTR(cpa_p0_rd_dat,	0xE2),
+	NULL
+};
+
+static const struct attribute_group hisi_cpa_pmu_events_group = {
+	.name = "events",
+	.attrs = hisi_cpa_pmu_events_attr,
+};
+
+static DEVICE_ATTR(cpumask, 0444, hisi_cpumask_sysfs_show, NULL);
+
+static struct attribute *hisi_cpa_pmu_cpumask_attrs[] = {
+	&dev_attr_cpumask.attr,
+	NULL
+};
+
+static const struct attribute_group hisi_cpa_pmu_cpumask_attr_group = {
+	.attrs = hisi_cpa_pmu_cpumask_attrs,
+};
+
+static struct device_attribute hisi_cpa_pmu_identifier_attr =
+	__ATTR(identifier, 0444, hisi_uncore_pmu_identifier_attr_show, NULL);
+
+static struct attribute *hisi_cpa_pmu_identifier_attrs[] = {
+	&hisi_cpa_pmu_identifier_attr.attr,
+	NULL
+};
+
+static const struct attribute_group hisi_cpa_pmu_identifier_group = {
+	.attrs = hisi_cpa_pmu_identifier_attrs,
+};
+
+static const struct attribute_group *hisi_cpa_pmu_attr_groups[] = {
+	&hisi_cpa_pmu_format_group,
+	&hisi_cpa_pmu_events_group,
+	&hisi_cpa_pmu_cpumask_attr_group,
+	&hisi_cpa_pmu_identifier_group,
+	NULL
+};
+
+static const struct hisi_uncore_ops hisi_uncore_cpa_pmu_ops = {
+	.write_evtype           = hisi_cpa_pmu_write_evtype,
+	.get_event_idx		= hisi_uncore_pmu_get_event_idx,
+	.start_counters		= hisi_cpa_pmu_start_counters,
+	.stop_counters		= hisi_cpa_pmu_stop_counters,
+	.enable_counter		= hisi_cpa_pmu_enable_counter,
+	.disable_counter	= hisi_cpa_pmu_disable_counter,
+	.enable_counter_int	= hisi_cpa_pmu_enable_counter_int,
+	.disable_counter_int	= hisi_cpa_pmu_disable_counter_int,
+	.write_counter		= hisi_cpa_pmu_write_counter,
+	.read_counter		= hisi_cpa_pmu_read_counter,
+	.get_int_status		= hisi_cpa_pmu_get_int_status,
+	.clear_int_status	= hisi_cpa_pmu_clear_int_status,
+};
+
+static int hisi_cpa_pmu_dev_probe(struct platform_device *pdev,
+				  struct hisi_pmu *cpa_pmu)
+{
+	int ret;
+
+	ret = hisi_cpa_pmu_init_data(pdev, cpa_pmu);
+	if (ret)
+		return ret;
+
+	ret = hisi_uncore_pmu_init_irq(cpa_pmu, pdev);
+	if (ret)
+		return ret;
+
+	cpa_pmu->counter_bits = CPA_COUNTER_BITS;
+	cpa_pmu->check_event = CPA_NR_EVENTS;
+	cpa_pmu->pmu_events.attr_groups = hisi_cpa_pmu_attr_groups;
+	cpa_pmu->ops = &hisi_uncore_cpa_pmu_ops;
+	cpa_pmu->num_counters = CPA_NR_COUNTERS;
+	cpa_pmu->dev = &pdev->dev;
+	cpa_pmu->on_cpu = -1;
+
+	return 0;
+}
+
+static int hisi_cpa_pmu_probe(struct platform_device *pdev)
+{
+	struct hisi_pmu *cpa_pmu;
+	char *name;
+	int ret;
+
+	cpa_pmu = devm_kzalloc(&pdev->dev, sizeof(*cpa_pmu), GFP_KERNEL);
+	if (!cpa_pmu)
+		return -ENOMEM;
+
+	ret = hisi_cpa_pmu_dev_probe(pdev, cpa_pmu);
+	if (ret)
+		return ret;
+
+	name = devm_kasprintf(&pdev->dev, GFP_KERNEL, "hisi_sicl%d_cpa%u",
+			      cpa_pmu->sicl_id, cpa_pmu->index_id);
+	if (!name)
+		return -ENOMEM;
+
+	cpa_pmu->pmu = (struct pmu) {
+		.name		= name,
+		.module		= THIS_MODULE,
+		.task_ctx_nr	= perf_invalid_context,
+		.event_init	= hisi_uncore_pmu_event_init,
+		.pmu_enable	= hisi_uncore_pmu_enable,
+		.pmu_disable	= hisi_uncore_pmu_disable,
+		.add		= hisi_uncore_pmu_add,
+		.del		= hisi_uncore_pmu_del,
+		.start		= hisi_uncore_pmu_start,
+		.stop		= hisi_uncore_pmu_stop,
+		.read		= hisi_uncore_pmu_read,
+		.attr_groups	= cpa_pmu->pmu_events.attr_groups,
+		.capabilities	= PERF_PMU_CAP_NO_EXCLUDE,
+	};
+
+	/* Power Management should be disabled before using CPA PMU. */
+	hisi_cpa_pmu_disable_pm(cpa_pmu);
+	ret = cpuhp_state_add_instance(CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE,
+				       &cpa_pmu->node);
+	if (ret) {
+		dev_err(&pdev->dev, "Error %d registering hotplug\n", ret);
+		hisi_cpa_pmu_enable_pm(cpa_pmu);
+		return ret;
+	}
+
+	ret = perf_pmu_register(&cpa_pmu->pmu, name, -1);
+	if (ret) {
+		dev_err(cpa_pmu->dev, "PMU register failed\n");
+		cpuhp_state_remove_instance_nocalls(
+			CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE, &cpa_pmu->node);
+		hisi_cpa_pmu_enable_pm(cpa_pmu);
+		return ret;
+	}
+
+	platform_set_drvdata(pdev, cpa_pmu);
+	return ret;
+}
+
+static int hisi_cpa_pmu_remove(struct platform_device *pdev)
+{
+	struct hisi_pmu *cpa_pmu = platform_get_drvdata(pdev);
+
+	perf_pmu_unregister(&cpa_pmu->pmu);
+	cpuhp_state_remove_instance_nocalls(CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE,
+					    &cpa_pmu->node);
+	hisi_cpa_pmu_enable_pm(cpa_pmu);
+	return 0;
+}
+
+static struct platform_driver hisi_cpa_pmu_driver = {
+	.driver = {
+		.name = "hisi_cpa_pmu",
+		.acpi_match_table = ACPI_PTR(hisi_cpa_pmu_acpi_match),
+		.suppress_bind_attrs = true,
+	},
+	.probe = hisi_cpa_pmu_probe,
+	.remove = hisi_cpa_pmu_remove,
+};
+
+static int __init hisi_cpa_pmu_module_init(void)
+{
+	int ret;
+
+	ret = cpuhp_setup_state_multi(CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE,
+				      "AP_PERF_ARM_HISI_CPA_ONLINE",
+				      hisi_uncore_pmu_online_cpu,
+				      hisi_uncore_pmu_offline_cpu);
+	if (ret) {
+		pr_err("setup hotplug failed: %d\n", ret);
+		return ret;
+	}
+
+	ret = platform_driver_register(&hisi_cpa_pmu_driver);
+	if (ret)
+		cpuhp_remove_multi_state(CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE);
+
+	return ret;
+}
+module_init(hisi_cpa_pmu_module_init);
+
+static void __exit hisi_cpa_pmu_module_exit(void)
+{
+	platform_driver_unregister(&hisi_cpa_pmu_driver);
+	cpuhp_remove_multi_state(CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE);
+}
+module_exit(hisi_cpa_pmu_module_exit);
+
+MODULE_DESCRIPTION("HiSilicon SoC CPA PMU driver");
+MODULE_LICENSE("GPL v2");
+MODULE_AUTHOR("Qi Liu <liuqi115@huawei.com>");
diff --git a/include/linux/cpuhotplug.h b/include/linux/cpuhotplug.h
index f4078abc061f..ee782c3cb7f3 100644
--- a/include/linux/cpuhotplug.h
+++ b/include/linux/cpuhotplug.h
@@ -158,6 +158,9 @@ enum cpuhp_state {
 	CPUHP_AP_PERF_S390_SF_ONLINE,
 	CPUHP_AP_PERF_ARM_CCI_ONLINE,
 	CPUHP_AP_PERF_ARM_CCN_ONLINE,
+	#ifndef __GENKSYMS__
+	CPUHP_AP_PERF_ARM_HISI_CPA_ONLINE,
+	#endif
 	CPUHP_AP_PERF_ARM_HISI_DDRC_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_HHA_ONLINE,
 	CPUHP_AP_PERF_ARM_HISI_L3_ONLINE,
-- 
2.27.0

