From 7b7d4988dfab6e6fc7fa3821aa0a015455171f83 Mon Sep 17 00:00:00 2001
From: liuxueping <liuxueping1@huawei.com>
Date: Sat, 29 Dec 2018 17:19:27 +0000
Subject: [PATCH] use tty0 other than ttyAMA0 in rescue mode

---
 share/templates.d/99-generic/config_files/aarch64/grub2-efi.cfg | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/share/templates.d/99-generic/config_files/aarch64/grub2-efi.cfg b/share/templates.d/99-generic/config_files/aarch64/grub2-efi.cfg
index 1cc389d..2f6fedb 100644
--- a/share/templates.d/99-generic/config_files/aarch64/grub2-efi.cfg
+++ b/share/templates.d/99-generic/config_files/aarch64/grub2-efi.cfg
@@ -40,7 +40,7 @@ submenu 'Troubleshooting -->' {
 		initrd @INITRDPATH@
 	}
 	menuentry 'Rescue a @PRODUCT@ system' --class red --class gnu-linux --class gnu --class os {
-		linux @KERNELPATH@ @ROOT@ rescue
+		linux @KERNELPATH@ @ROOT@ rescue console=ttyAMA0 console=tty0
 		initrd @INITRDPATH@
 	}
 }
-- 
1.8.3.1

