From ee8de09f5b23c067f991f55d4f4ae6a6dc6de11c Mon Sep 17 00:00:00 2001
From: Richard Henderson <richard.henderson@linaro.org>
Date: Sat, 8 Feb 2020 12:57:59 +0000
Subject: [PATCH] target/arm: Add isar_feature tests for PAN + ATS1E1
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Include definitions for all of the bits in ID_MMFR3.
We already have a definition for ID_AA64MMFR1.PAN.

Reviewed-by: Alex Bennée <alex.bennee@linaro.org>
Reviewed-by: Peter Maydell <peter.maydell@linaro.org>
Signed-off-by: Richard Henderson <richard.henderson@linaro.org>
Message-id: 20200208125816.14954-4-richard.henderson@linaro.org
Signed-off-by: Peter Maydell <peter.maydell@linaro.org>
(cherry-picked from commit 3d6ad6bb466f487bcc861f99e2c9054230df1076)
Signed-off-by: Peng Liang <liangpeng10@huawei.com>
---
 target/arm/cpu.h | 29 +++++++++++++++++++++++++++++
 1 file changed, 29 insertions(+)

diff --git a/target/arm/cpu.h b/target/arm/cpu.h
index 86eb79cd02..fe3108281a 100644
--- a/target/arm/cpu.h
+++ b/target/arm/cpu.h
@@ -1680,6 +1680,15 @@ FIELD(ID_ISAR6, FHM, 8, 4)
 FIELD(ID_ISAR6, SB, 12, 4)
 FIELD(ID_ISAR6, SPECRES, 16, 4)
 
+FIELD(ID_MMFR3, CMAINTVA, 0, 4)
+FIELD(ID_MMFR3, CMAINTSW, 4, 4)
+FIELD(ID_MMFR3, BPMAINT, 8, 4)
+FIELD(ID_MMFR3, MAINTBCST, 12, 4)
+FIELD(ID_MMFR3, PAN, 16, 4)
+FIELD(ID_MMFR3, COHWALK, 20, 4)
+FIELD(ID_MMFR3, CMEMSZ, 24, 4)
+FIELD(ID_MMFR3, SUPERSEC, 28, 4)
+
 FIELD(ID_MMFR4, SPECSEI, 0, 4)
 FIELD(ID_MMFR4, AC2, 4, 4)
 FIELD(ID_MMFR4, XNX, 8, 4)
@@ -3445,6 +3454,16 @@ static inline bool isar_feature_aa32_vminmaxnm(const ARMISARegisters *id)
     return FIELD_EX64(id->mvfr2, MVFR2, FPMISC) >= 4;
 }
 
+static inline bool isar_feature_aa32_pan(const ARMISARegisters *id)
+{
+    return FIELD_EX64(id->mvfr0, ID_MMFR3, PAN) != 0;
+}
+
+static inline bool isar_feature_aa32_ats1e1(const ARMISARegisters *id)
+{
+    return FIELD_EX64(id->mvfr0, ID_MMFR3, PAN) >= 2;
+}
+
 /*
  * 64-bit feature tests via id registers.
  */
@@ -3589,6 +3608,16 @@ static inline bool isar_feature_aa64_lor(const ARMISARegisters *id)
     return FIELD_EX64(id->id_aa64mmfr1, ID_AA64MMFR1, LO) != 0;
 }
 
+static inline bool isar_feature_aa64_pan(const ARMISARegisters *id)
+{
+    return FIELD_EX64(id->id_aa64mmfr1, ID_AA64MMFR1, PAN) != 0;
+}
+
+static inline bool isar_feature_aa64_ats1e1(const ARMISARegisters *id)
+{
+    return FIELD_EX64(id->id_aa64mmfr1, ID_AA64MMFR1, PAN) >= 2;
+}
+
 static inline bool isar_feature_aa64_bti(const ARMISARegisters *id)
 {
     return FIELD_EX64(id->id_aa64pfr1, ID_AA64PFR1, BT) != 0;
-- 
2.23.0

