From 3602361df4f43e4e5d5dc56e9e767ee93b8176bd Mon Sep 17 00:00:00 2001
From: Peter Maydell <peter.maydell@linaro.org>
Date: Fri, 14 Feb 2020 17:51:04 +0000
Subject: [PATCH] target/arm: Add _aa64_ and _any_ versions of pmu_8_1 isar
 checks
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add the 64-bit version of the "is this a v8.1 PMUv3?"
ID register check function, and the _any_ version that
checks for either AArch32 or AArch64 support. We'll use
this in a later commit.

We don't (yet) do any isar_feature checks on ID_AA64DFR1_EL1,
but we move id_aa64dfr1 into the ARMISARegisters struct with
id_aa64dfr0, for consistency.

Reviewed-by: Richard Henderson <richard.henderson@linaro.org>
Reviewed-by: Philippe Mathieu-Daudé <philmd@redhat.com>
Signed-off-by: Peter Maydell <peter.maydell@linaro.org>
Message-id: 20200214175116.9164-10-peter.maydell@linaro.org
(cherry-picked from commit 2a609df87d9b886fd38a190a754dbc241ff707e8)
Signed-off-by: Peng Liang <liangpeng10@huawei.com>
---
 target/arm/cpu.c    |  3 ++-
 target/arm/cpu.h    | 15 +++++++++++++--
 target/arm/cpu64.c  |  8 ++++----
 target/arm/helper.c | 12 +++++++-----
 4 files changed, 26 insertions(+), 12 deletions(-)

diff --git a/target/arm/cpu.c b/target/arm/cpu.c
index 7e9b85a289..bb2edf4e18 100644
--- a/target/arm/cpu.c
+++ b/target/arm/cpu.c
@@ -1522,7 +1522,8 @@ static void arm_cpu_realizefn(DeviceState *dev, Error **errp)
                 cpu);
 #endif
     } else {
-        cpu->id_aa64dfr0 = FIELD_DP64(cpu->id_aa64dfr0, ID_AA64DFR0, PMUVER, 0);
+        cpu->isar.id_aa64dfr0 =
+            FIELD_DP64(cpu->isar.id_aa64dfr0, ID_AA64DFR0, PMUVER, 0);
         cpu->isar.id_dfr0 = FIELD_DP32(cpu->isar.id_dfr0, ID_DFR0, PERFMON, 0);
         cpu->pmceid0 = 0;
         cpu->pmceid1 = 0;
diff --git a/target/arm/cpu.h b/target/arm/cpu.h
index 2d8d27e80a..230130be81 100644
--- a/target/arm/cpu.h
+++ b/target/arm/cpu.h
@@ -868,6 +868,8 @@ struct ARMCPU {
         uint64_t id_aa64mmfr0;
         uint64_t id_aa64mmfr1;
         uint64_t id_aa64mmfr2;
+        uint64_t id_aa64dfr0;
+        uint64_t id_aa64dfr1;
     } isar;
     uint32_t midr;
     uint32_t revidr;
@@ -884,8 +886,6 @@ struct ARMCPU {
     uint32_t id_mmfr2;
     uint32_t id_mmfr3;
     uint32_t id_mmfr4;
-    uint64_t id_aa64dfr0;
-    uint64_t id_aa64dfr1;
     uint64_t id_aa64afr0;
     uint64_t id_aa64afr1;
     uint32_t dbgdidr;
@@ -3657,6 +3657,17 @@ static inline bool isar_feature_aa64_bti(const ARMISARegisters *id)
     return FIELD_EX64(id->id_aa64pfr1, ID_AA64PFR1, BT) != 0;
 }
 
+static inline bool isar_feature_aa64_pmu_8_1(const ARMISARegisters *id)
+{
+    return FIELD_EX64(id->id_aa64dfr0, ID_AA64DFR0, PMUVER) >= 4 &&
+        FIELD_EX64(id->id_aa64dfr0, ID_AA64DFR0, PMUVER) != 0xf;
+}
+
+static inline bool isar_feature_any_pmu_8_1(const ARMISARegisters *id)
+{
+    return isar_feature_aa64_pmu_8_1(id) || isar_feature_aa32_pmu_8_1(id);
+}
+
 /*
  * Forward to the above feature tests given an ARMCPU pointer.
  */
diff --git a/target/arm/cpu64.c b/target/arm/cpu64.c
index afdabbebbf..aa96548f10 100644
--- a/target/arm/cpu64.c
+++ b/target/arm/cpu64.c
@@ -137,7 +137,7 @@ static void aarch64_a57_initfn(Object *obj)
     cpu->isar.id_isar5 = 0x00011121;
     cpu->isar.id_isar6 = 0;
     cpu->isar.id_aa64pfr0 = 0x00002222;
-    cpu->id_aa64dfr0 = 0x10305106;
+    cpu->isar.id_aa64dfr0 = 0x10305106;
     cpu->isar.id_aa64isar0 = 0x00011120;
     cpu->isar.id_aa64mmfr0 = 0x00001124;
     cpu->dbgdidr = 0x3516d000;
@@ -191,7 +191,7 @@ static void aarch64_a53_initfn(Object *obj)
     cpu->isar.id_isar5 = 0x00011121;
     cpu->isar.id_isar6 = 0;
     cpu->isar.id_aa64pfr0 = 0x00002222;
-    cpu->id_aa64dfr0 = 0x10305106;
+    cpu->isar.id_aa64dfr0 = 0x10305106;
     cpu->isar.id_aa64isar0 = 0x00011120;
     cpu->isar.id_aa64mmfr0 = 0x00001122; /* 40 bit physical addr */
     cpu->dbgdidr = 0x3516d000;
@@ -244,7 +244,7 @@ static void aarch64_a72_initfn(Object *obj)
     cpu->isar.id_isar4 = 0x00011142;
     cpu->isar.id_isar5 = 0x00011121;
     cpu->isar.id_aa64pfr0 = 0x00002222;
-    cpu->id_aa64dfr0 = 0x10305106;
+    cpu->isar.id_aa64dfr0 = 0x10305106;
     cpu->isar.id_aa64isar0 = 0x00011120;
     cpu->isar.id_aa64mmfr0 = 0x00001124;
     cpu->dbgdidr = 0x3516d000;
@@ -276,7 +276,7 @@ static void aarch64_kunpeng_920_initfn(Object *obj)
     cpu->midr = 0x480fd010;
     cpu->ctr = 0x84448004;
     cpu->isar.id_aa64pfr0 = 0x11001111;
-    cpu->id_aa64dfr0 = 0x110305408;
+    cpu->isar.id_aa64dfr0 = 0x110305408;
     cpu->isar.id_aa64isar0 = 0x10211120;
     cpu->isar.id_aa64mmfr0 = 0x101125;
 }
diff --git a/target/arm/helper.c b/target/arm/helper.c
index 3f06ca1964..a71f4ef62d 100644
--- a/target/arm/helper.c
+++ b/target/arm/helper.c
@@ -23,6 +23,7 @@
 #include "hw/semihosting/semihost.h"
 #include "sysemu/cpus.h"
 #include "sysemu/kvm.h"
+#include "sysemu/tcg.h"
 #include "qemu/range.h"
 #include "qapi/qapi-commands-machine-target.h"
 #include "qapi/error.h"
@@ -5611,9 +5612,10 @@ static void define_debug_regs(ARMCPU *cpu)
      * check that if they both exist then they agree.
      */
     if (arm_feature(&cpu->env, ARM_FEATURE_AARCH64)) {
-        assert(FIELD_EX64(cpu->id_aa64dfr0, ID_AA64DFR0, BRPS) == brps);
-        assert(FIELD_EX64(cpu->id_aa64dfr0, ID_AA64DFR0, WRPS) == wrps);
-        assert(FIELD_EX64(cpu->id_aa64dfr0, ID_AA64DFR0, CTX_CMPS) == ctx_cmps);
+        assert(FIELD_EX64(cpu->isar.id_aa64dfr0, ID_AA64DFR0, BRPS) == brps);
+        assert(FIELD_EX64(cpu->isar.id_aa64dfr0, ID_AA64DFR0, WRPS) == wrps);
+        assert(FIELD_EX64(cpu->isar.id_aa64dfr0, ID_AA64DFR0, CTX_CMPS)
+               == ctx_cmps);
     }
 
     define_one_arm_cp_reg(cpu, &dbgdidr);
@@ -6112,11 +6114,11 @@ void register_cp_regs_for_features(ARMCPU *cpu)
             { .name = "ID_AA64DFR0_EL1", .state = ARM_CP_STATE_AA64,
               .opc0 = 3, .opc1 = 0, .crn = 0, .crm = 5, .opc2 = 0,
               .access = PL1_R, .type = ARM_CP_CONST,
-              .resetvalue = cpu->id_aa64dfr0 },
+              .resetvalue = cpu->isar.id_aa64dfr0 },
             { .name = "ID_AA64DFR1_EL1", .state = ARM_CP_STATE_AA64,
               .opc0 = 3, .opc1 = 0, .crn = 0, .crm = 5, .opc2 = 1,
               .access = PL1_R, .type = ARM_CP_CONST,
-              .resetvalue = cpu->id_aa64dfr1 },
+              .resetvalue = cpu->isar.id_aa64dfr1 },
             { .name = "ID_AA64DFR2_EL1_RESERVED", .state = ARM_CP_STATE_AA64,
               .opc0 = 3, .opc1 = 0, .crn = 0, .crm = 5, .opc2 = 2,
               .access = PL1_R, .type = ARM_CP_CONST,
-- 
2.23.0

