From b728ea5f2597f97088db8517576caa2877118cb0 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Marc-Andr=C3=A9=20Lureau?= <marcandre.lureau@redhat.com>
Date: Mon, 5 Aug 2019 16:04:40 +0800
Subject: [PATCH] virtio-pci: fix missing device properties
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Since commit a4ee4c8baa37154 ("virtio: Helper for registering virtio
device types"), virtio-gpu-pci, virtio-vga, and virtio-crypto-pci lost
some properties: "ioeventfd" and "vectors". This may cause various
issues, such as failing migration or invalid properties.

Since those VirtioPCI devices do not have a base name, their class are
initialized with virtio_pci_generic_base_class_init(). However, if the
VirtioPCIDeviceTypeInfo provided a class_init which sets dc->props,
the properties were overwritten by virtio_pci_generic_class_init().

Instead, introduce an intermediary base-type to register the generic
properties.

Fixes: a4ee4c8baa37154f42b4dc6a13fee79268d15238
Cc: qemu-stable@nongnu.org
Signed-off-by: Marc-André Lureau <marcandre.lureau@redhat.com>
Message-Id: <20190625232333.30752-1-marcandre.lureau@redhat.com>
(cherry-pick from commit 683c1d89efd1eeb111c129a9a91f629b94d90d45)
---
 hw/virtio/virtio-pci.c | 28 ++++++++++++++--------------
 1 file changed, 14 insertions(+), 14 deletions(-)

diff --git a/hw/virtio/virtio-pci.c b/hw/virtio/virtio-pci.c
index cb44e19b..497092e8 100644
--- a/hw/virtio/virtio-pci.c
+++ b/hw/virtio/virtio-pci.c
@@ -1905,13 +1905,6 @@ static void virtio_pci_generic_class_init(ObjectClass *klass, void *data)
     dc->props = virtio_pci_generic_properties;
 }
 
-/* Used when the generic type and the base type is the same */
-static void virtio_pci_generic_base_class_init(ObjectClass *klass, void *data)
-{
-    virtio_pci_base_class_init(klass, data);
-    virtio_pci_generic_class_init(klass, NULL);
-}
-
 static void virtio_pci_transitional_instance_init(Object *obj)
 {
     VirtIOPCIProxy *proxy = VIRTIO_PCI(obj);
@@ -1930,14 +1923,13 @@ static void virtio_pci_non_transitional_instance_init(Object *obj)
 
 void virtio_pci_types_register(const VirtioPCIDeviceTypeInfo *t)
 {
+    char *base_name = NULL;
     TypeInfo base_type_info = {
         .name          = t->base_name,
         .parent        = t->parent ? t->parent : TYPE_VIRTIO_PCI,
         .instance_size = t->instance_size,
         .instance_init = t->instance_init,
         .class_size    = t->class_size,
-        .class_init    = virtio_pci_base_class_init,
-        .class_data    = (void *)t,
         .abstract      = true,
     };
     TypeInfo generic_type_info = {
@@ -1953,13 +1945,20 @@ void virtio_pci_types_register(const VirtioPCIDeviceTypeInfo *t)
 
     if (!base_type_info.name) {
         /* No base type -> register a single generic device type */
-        base_type_info.name = t->generic_name;
-        base_type_info.class_init = virtio_pci_generic_base_class_init;
-        base_type_info.interfaces = generic_type_info.interfaces;
-        base_type_info.abstract = false;
-        generic_type_info.name = NULL;
+        /* use intermediate %s-base-type to add generic device props */
+        base_name = g_strdup_printf("%s-base-type", t->generic_name);
+        base_type_info.name = base_name;
+        base_type_info.class_init = virtio_pci_generic_class_init;
+
+        generic_type_info.parent = base_name;
+        generic_type_info.class_init = virtio_pci_base_class_init;
+        generic_type_info.class_data = (void *)t;
+
         assert(!t->non_transitional_name);
         assert(!t->transitional_name);
+    } else {
+        base_type_info.class_init = virtio_pci_base_class_init;
+        base_type_info.class_data = (void *)t;
     }
 
     type_register(&base_type_info);
@@ -1997,6 +1996,7 @@ void virtio_pci_types_register(const VirtioPCIDeviceTypeInfo *t)
         };
         type_register(&transitional_type_info);
     }
+    g_free(base_name);
 }
 
 /* virtio-pci-bus */
-- 
2.19.1

