From a0b1a84acf061473902e6fa2abf848e2ff537513 Mon Sep 17 00:00:00 2001
From: Jian Shen <shenjian15@huawei.com>
Date: Tue, 27 Jul 2021 15:10:37 +0800
Subject: [PATCH 095/283] net: hns3: fix rx VLAN offload state inconsistent
 issue

mainline inclusion
from mainline-v5.14-rc3
commit bbfd4506f962e7e6fff8f37f017154a3c3791264
category: bugfix
bugzilla: https://gitee.com/src-openeuler/kernel/issues/I8EMUR
CVE: NA

Reference: https://git.kernel.org/pub/scm/linux/kernel/git/torvalds/linux.git/commit/?id=bbfd4506f962e7e6fff8f37f017154a3c3791264

----------------------------------------------------------------------

Currently, VF doesn't enable rx VLAN offload when initializating,
and PF does it for VFs. If user disable the rx VLAN offload for
VF with ethtool -K, and reload the VF driver, it may cause the
rx VLAN offload state being inconsistent between hardware and
software.

Fixes it by enabling rx VLAN offload when VF initializing.

Fixes: e2cb1dec9779 ("net: hns3: Add HNS3 VF HCL(Hardware Compatibility Layer) Support")
Signed-off-by: Jian Shen <shenjian15@huawei.com>
Signed-off-by: Guangbin Huang <huangguangbin2@huawei.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
Reviewed-by: Yongxin Li <liyongxin1@huawei.com>
Signed-off-by: Junxin Chen <chenjunxin1@huawei.com>
Signed-off-by: Zheng Zengkai <zhengzengkai@huawei.com>
Signed-off-by: Xiaodong Li <lixiaodong67@huawei.com>
---
 .../net/ethernet/hisilicon/hns3/hns3vf/hclgevf_main.c  | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_main.c b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_main.c
index d58b4e4780a8..4cab9c19031a 100644
--- a/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_main.c
+++ b/drivers/net/ethernet/hisilicon/hns3/hns3vf/hclgevf_main.c
@@ -2569,6 +2569,16 @@ static int hclgevf_rss_init_hw(struct hclgevf_dev *hdev)
 
 static int hclgevf_init_vlan_config(struct hclgevf_dev *hdev)
 {
+	struct hnae3_handle *nic = &hdev->nic;
+	int ret;
+
+	ret = hclgevf_en_hw_strip_rxvtag(nic, true);
+	if (ret) {
+		dev_err(&hdev->pdev->dev,
+			"failed to enable rx vlan offload, ret = %d\n", ret);
+		return ret;
+	}
+
 	return hclgevf_set_vlan_filter(&hdev->nic, htons(ETH_P_8021Q), 0,
 				       false);
 }
-- 
2.34.1

